========
Newsgroups: comp.sys.cbm
Subject: COMP.SYS.CBM: General FAQ, v3.1 Part 1/9
From: brain@mail.msen.com (Jim Brain)
Date: 13 Aug 1996 00:27:44 -0400


X-Posted-By: YPost, version 0.08


Archive-name: cbm-main-faq.3.1.p1
Comp-answers-archive-name: commodore/main-faq/part1
News-answers-archive-name: commodore/main-faq/part1
Comp-sys-cbm-archive-name: main-faq/part1
Version: 3.1
Last-modified: 1996/08/12
		       	

  Disclaimer: 
  
| This file is maintained by Jim Brain (brain@mail.msen.com, j.brain@ieee.org,
| brain@acm.org).  It is composed of information gleaned from articles in the 
| USENET newsgroup comp.sys.cbm, the FidoNET echoes CBM and CBM-128,
| electronic mail messages, World Wide Web pages, and othee authors have either directly or indirectly given their consent to use 
| their work in this FAQ.  All of the information in this file has been 
| gathered and checked if possibl of any statement in this file.  If in doubt, please bring up 
| the subject in one of the Commodore forums.
  
| If you have suggestions, comments, or criticisms, please let Jim Brain
| know by sending electronic mail to brain@mail.msen.com.  If, you find that
| address no longer available, please try the forwarding accounts
| j.brain@ieee.org or brain@acm.org.  Keep in mind that new questions appear
| on a daily basis, so there is a finite time between a new question 
| appearing in comp.sys.cbm, and its inclusion in this file.

  The latest version of this file may be obtained from the following places:
  
  ftp sites:
    ftp://ccnga.uwaterloo.ca/pub/cbm/comp.sys.cbm/cbm-main-faq.3.1
    ftp://ftp.funet.fi/pub/cbm/faq/cbm-main-faq.3.1.gz
    ftp://rtfm.mit.edu/pub/usenet/comp.sys.cbm/main-faq/part*
    ftp://rtfm.mit.edu/pub/usenet/news.answers/commodore/main-faq/part*
    ftp://rtfm.mit.edu/pub/usenet/comp.answers/commodore/main-faq/part*
    ftp://bbs.cc.uniud.it/pub/c64/comp.sys.cbm/faq.zip
    ftp://ftp.armory.com/pub/user/spectre/TEXT-ARCHIVE/comp.sys.cbm.faq.3.1.gz

  World Wide Web sites:
    http://www.msen.com/~brain/faqhome.html

  Bulletin Board Systems:
|   COMMODORE CEE BBS (916) 339-3403,               FIDONET address: 1:203/999
|   VGA Cologne BBS   +49-221-9808007 (19.2 ZyXel/ISDN) 
|                            -9808008 (28.8 V.FC/ISDN)
|                                                   FidoNET address						      
  Mailservers:
    mail-server@rtfm.mit.edu.  First nine lines of message:
      send /usenet/comp.sys.cbm/main-faq/part1
      send /usenet/comp.sys.cbm/main-faq/part2
      sensend /usenet/comp.sys.cbm/main-faq/part4
      send /usenet/comp.sys.cbm/main-faq/part5
      send /usenet/comp.sys.cbm/main-faq/part6
      send /usenet/comp.sys.cbm/main-faq/part7
      send /usenet/comp.sys.cbm/main-faq/part8
      send /usenet/comp.sys.cbm/main-faq/part9
    
  brain@mail.msen.com (Jim Brain's Mailserver - always has latest copy)
    Subject: MAILSERV
      send faq.p*
      
  Mailing List  
    To receive any major updates to the FAQ, mail:
      To: brain@mail.msen.com
      Subject: MAILSERV
      Body:
      subscribe cbm-main-faq Firstname Lastname
      quit
      
  See Section 6 for directions on how to use these services to retrieve the
  FAQ.

  This file is posted to the groups comp.sys.cbm, news.answers, and
| comp.answers once every month around the 5th of the month.
                            
  _Notes for this release_:
  -----------------------
  
+ Still left to add.  Maybe next time....
  rewrite  of section 13.8.
  a section devoted to downloading software (maybe)
  changes to section 12.3 to detail hooking up monitors.
  
  Most notable changes include removing many long lists, and splitting
  the FAQ into 9 < 32kB pieces.
   
  I am gathering a list of Commodore reference books together.  If you
  have a book, please send me the ISBN, Author, TItle, short description,
  number of pages, whether it has illustrations, and wh  any code samples.  Thanks.

  -----------------------

  Lines preceded with a '|" have been modified since the last version of this
  file was posted.  Lines preceded by a '+' have been added since the last
  version was posted.

  If readers of this FAQ wish to make changes, please precede formatted lines
  sent to me with a 'C' so that I can see the changes even if you enclose
  header and trailer text to show context.

  ---------------------------------------------------------------------------


  Table of Contents
  -----------------

   1.  Introduction
   1.1.  What is a FAQ
   1.2.  What topics does this FAQ cover?
   1.3.  Who decides what goes in the FAQ?
   1.4.  How do I retrieve updates to the FAQ?
  
   2.  Overview
   2.1.  Do people still use Commodore 8-bit machines?
   2.2.  How many Commodore machines are there?
   2.3.  What do people do with Commodore 8-bit machines?
   2.4.  What Commodore 8-bit machines are most widely used?
   2.5.  What is the economic status of Commodore?
   
   3.  The BASICs
   3.1.  How do I format a Commodore disk?
   3.2.  How do I transform a BASIC program to a text file?
   3.3.  How do I transform a text file into a BASIC program?
   3.4.  How can I change my dsoftware?
   3.5.  Can I get my 1581 drive to change its device number on startup?
  
   4.  Publications
   4.1.  What paper publications are available?
   4.2.  What paper publications have disappeared?
   4.3.  What is a Disk Magazine?  Where do I find them?
   4.4.  What is an Online Magazine?  Where do I find them?
   4.5.  Are there other publications I should be aware of?
   4.6.  How do I know which magazines to subscribe to?
   
   5.  Connecting Up
   5.1.  How do I connect my computer to the outside world?
   5.2.  What services can I use to get online?
   5.3.  What hardware do I need?
   5.4.  What kinds of terminal programs exist?
   5.4.1.  What kinds of terminal programs exist for the 64?
   5.4.2.  What kinds of terminal programs exist for the 128?
   5.5.  Can I use my Commodore computer on Amateur Radio?
   5.6.  Is there TCP/IP software available for Commodore computers?
   
   6.  The Online Information Reservoir
   6.1.  How do I download?  What is a transfer protocol?
   6.2.  What is the difference between PETSCII and ASCII?
   6.3.  Where can I find Commodore programs?
   6.4.  What is a file extension, and what do they stand for?
   6.5.  What is electronic mail?
   6.5.1.  What are mailing lists 6.5.2.  What is a Mail Server?  How do I use one?
   6.5.3.  How do I contact people on Compuserve, Genie, etc.?
   6.6.  What is USENET or NetNews?  What is a USENET newsgroup?
   6.6.1.  What news groups cater to Commodore 8-bit machines? 
   6.6.2.  What types of discussions belong in comp.sys.cbm?
   6.6.3.  Which issues does comp.sys.cbm discuss regularly?
   6.6.4.  How do I post in comp.sys.cbm?
   6.6.5.  How can I access comp.sys.cbm through email?
+  6.6.6.  How can I read comp.sys.cbm through WWW?
   6.7.  What is a FidoNET echo?
   6.7.1.  What echoes cater to Commodore 8-bit machines? 
   6.7.2.  How do I post in an echo?
   6.8.  What is the World Wide Web?
   6.8.1.  What WWW sites have Commodore information?
   6.8.2.  What Sites have Telnet WWW Browsers?
   6.9.  What is File Transfer Protocol (FTP)?
   6.9.1.  What FTP sites have Commodore Information?
   6.9.2.  What is an FTP Mail Server?  How do I use one?
   6.9.3.  How do I send files to an FTP site?
   6.10. What is Internet Relay Chat (IRC)?
   6.11. What else is available online?
    
   7.  Exchanging Data
   7.1.  How do I exchange data among Commodore 8-bit machines?
   7.2.  How do I exchange data between an IBM(tm) and my Commodore?
   7.3.  How do I exchange data betwee and my Commodore?
   7.4.  How do I exchange data between a Macintosh(tm) and my Commodore?
   7.5.  How do I exchange data between an Atari ST(tm) and my Commodore?
   7.6.  How do I exchange data between a UNIX(tm) machine and my Commodore?
   7.7.  Are there other ways to exchange data between computers?

   8.  Operating Systems
   8.1.  What Operating Systems are available?
   8.2.  What is GEOS?
   8.3.  What is UNIX?
   8.4.  What is CP/M

   9.  Demonstrations
   9.1.  Just what is a demonstration, or demo?
   9.2.  What does NTSC and PAL mean?
   9.3.  Where do I get demos?
   9.4.  What is a demo competition?
   9.5   What does FLI, DYCP, etc. mean?

  10.  Emulators
  10.1.  What is an emulator?
  10.2.  What platforms do 64 emulators exist on?
  10.3.  What platforms do 128 emulators exist on?
  10.4.  Are any other Commodore computers emulated?

  11.  Troubleshooting
  11.1.  What do I do for my ill disk drive?
  11.2.  What do I do for my ill computer?
  11.2.1.  What do I do for my ill Commodore 64?
  11.2.2.  What do I do for my ill Commodore 128?
  11.3.  What do I do for my ill keyboard?
  
  12.  Modifications and Cabling
  12.1.  How can you alter which side a 1571 reads from?
  12.2.  How do I open a C128 power supply?
  12.3.  How do I make a cable to hook my CBM 1902A to my 64 or 128?
  12.4.  How dole RS-232 interface cable?
  12.5.  How do I build a 2400/9600 bps RS-232 interface cable?
  12.6.  How can I determine how much VDC video memory is in my C128?
  12.7.  How do I build a GEOCable interface?
+ 12.8.  How do I connect my Commodore printer to an IBM PC?
  
  13.  Enhancements
  13.1.  How do I increase my disk drive's transfer speed?
  13.1.1.  What is a Fastloader?
  13.1.2.  What is a ROM replacement?
  13.1.3.  What are the disadvantages to using a drive enhancement?
  13.1.4.  What other things can I do to speed up the drive?
  13.2.  How do I expand my disk drive's capacity?
  13.2.1.  What is a Hard Drive?  Who sells them?
  13.2.2.  What is 64NET?
+ 13.2.3.  What is SERVER64?
  13.3.  How do I expand my computer's RAM capacity?
  13.3.1.  What is a Ram Expansion Unit?
  13.3.2.  What is a geoRAM Unit?
  13.3.3.  What is battery backed GeoRAM (BBGRam)?
  13.3.4.  What is a RAMLink?
  13.3.5.  What is a RAMDrive?
  13.3.6.  How do I expand my C128 Video RAM?
  13.3.7.  How do I expand my C64 internally?
  13.3.8.  How do I expand my C128 internally?
  13.4.  How do I increase my computer's speed?
  13.4.1.  How do I increase my Commodore 64's speed?
  13.4.2.  How do I increase my Commodore 128's speed?
  13.4.3.  Can I speed up other Commodore computers?
  13.5.  How do I iscreen's resolution?
  13.5.1.  How do I increase my Commodore 64's screen resolution?
  13.5.2.  How do I increase my Commodore 128's screen resolution?
  13.5.3.  How do I increase other CBM computers' resolutions?
  13.6.  How do I increase my computer's serial transfer speed?
  13.7.  How do I increase my computer's sound quality?
  13.8.  What other ways can I expand my Commodore computer?
   
  14.  Programming
  14.1.  What Programming Languages are available?
  14.2.  What is a Cross Assembler?  How do I use one?
  14.3   What is an "undocumented opcode"?
   
  15.  User Groups

  16.  Sales and Service
  16.1.  Where do I purchase Commodore Equipment and Software?
  16.2.  Where do I get equipment serviced?
  16.3.  How do I know who to buy from or request service from?
   
  17. Miscellaneous
  17.1.  How fast does a Commodore 64 run?
  17.2.  How can a turn my NTSC-M 64 into a PAL-B 64 or vice versa?
  17.3.  What does this IC number mean?
+ 17.4.  What are the differences between C64 ROM Revisions?
     
  18. Credits   
   
  ---------------------------------------------------------------------------


   1. Introduction

  Welcome to the comp.sys.cbm "Frequently Asked Questions" (FAQ) file.
  Many news groups maintain a FAQ file which is posted monthly, and
  is a repository for general interest and common information thers of the news group, or new readers of the news group, might be
  interested in.
  
  
   1.1.  What is a FAQ
   
  FAQ is an acronym that stands for "Frequently Asked Questions".  Shortly
  after the introduction of USENET, many people noticed that certain
  questions were repeatedly asked in newsgroups.  To minimize the posting of
  answers to already answered questions, USENET developed the idea of FAQ
  files.  After a question has been asked a number of times in the USENET
  newsgroup, it is added to the list of answered questions in the FAQ. 
  Then, readers are encouraged to read the FAQ to cut down on posts of
  repeated questions.  
  
  A FAQ file is not solely for newcomers.  Experienced users are encouraged
  to glance over the FAQ every so often to check for errors and add items.
  Also, it seems that everyone gets a question answered by reading the FAQ,
  new user or not.
   
   
   1.2.  What topics does this FAQ cover?
   
  This FAQ answers questions on just about any topic concerning Commodore
  computers.  Obviously, given the nature of the FAQ file, it is impossible
  to answer every question here, and some topics are too broad for discussion
  in the FAQ.  However, when thnnot adequately answer a question, it
  does provide pointers to relevant people or materials.
  
  Even though a large number of people use their Commodore computer to
  program, the topic is much too broad for adequate coverage in the FAQ.  For
  those interested in programming, however, please see Section 14, 
  "Programming".

   
   1.3.  Who decides what goes in the FAQ?
   
  Typically, a FAQ file is editted by a single person or small group of
  people.  These editors decide what should go into the FAQ.  Obviously,
  for the FAQ to fulfill its intended purpose, any question that has been
  asked repeatedly should be included, as should updates to any questions
  already in the FAQ.  The FAQ maintainer should try to provide as 
  up-to-date information as possible in the FAQ.  Above that, the FAQ
  maintainer can include any other information he or she deems or interest
  or value to the readers.
  
  For this FAQ, the FAQ maintainer is Jim Brain, brain@mail.msen.com, 
  j.brain@ieee.org, or brain@acm.org.
  
  If you have information that you feel should be included, please mail
  it to Jim.  Please be aware that it does take time to include new
  information.
   
   
   1.4.  How do I retrieve updates to the FAQ?

| The FAQ is posted on the 20th of the month to the USENET newsgroup 
| comp.sys.cbm.  It is automatically archived on the FTP site 
| rtfm.mit.edu and automatically archived on Jim Brain's mailserver.
  Most Bulletin Board Systems and Usert copy of the
  FAQ, and numerous magazines and other publications have included parts
  or all of the FAQ on disk or in print in recent months.  This FAQ is
  called the "COMP.SYS.CBM General Frequently Asked Questions List".
 
  The latest version of this file may be obtained from the following places:
  
  ftp sites:
    ftp://ccnga.uwaterloo.ca/pub/cbm/comp.sys.cbm/cbm-main-faq.3.1
    ftp://ftp.funet.fi/pub/cbm/faq/cbm-main-faq.3.1.gz
    ftp://rtfm.mit.edu/pub/usenet/comp.sys.cbm/main-faq/part*
    ftp://rtfm.mit.edu/pub/usenet/news.answers/commodore/main-faq/part*
    ftp://rtfm.mit.edu/pub/usenet/comp.answers/commodore/main-faq/part*
    ftp://bbs.cc.uniud.it/pub/c64/comp.sys.cbm/faq.zip
    ftp://ftp.armory.com/pub/user/spectre/TEXT-ARCHIVE/comp.sys.cbm.faq.3.1.gz

  World Wide Web sites:
    http://www.msen.com/~brain/faqhome.html

  Bulletin Board Systems:
|   COMMODORE CEE BBS 3,               FIDONET address: 1:203/999
|   VGA Cologne BBS   +49-221-9808007 (19.2 ZyXel/ISDN) 
|                            -9808008 (28.8 V.F                                          FidoNET address 2:2450/140

  Mailservers:
    mail-server@rtfm.mit.edu.  First nine lines of message:
      send /usenet/comp.sys.cbm/main-faq/part1
      send /usenet/comp.sys.cbm/main-faq/part2
      send /usenet/comp.sys.cbm/main-faq/part3
      send /usenet/comp.sys.cbm/main-faq/part4
      send /usenet/comp.sys.cbm/main-faq/part5
      send /usenet/comp.sys.cbm/main-faq/part6
      send /usenet/comp.sys.cbm/main-faq/part7
      send /usenet/comp.sys.cbm/main-faq/part8
      send /usenet/comp.sys.cbm/main-faq/part9
    
  brain@mail.msen.com (Jim Brain's Mailserver - always has latest copy)
    Subject: MAILSERV
      send faq.p*
      
  Mailing List  
    To receive any major updates to the FAQ, mail:
      To: brain@mail.msen.com
      Subject: MAILSERV
      Body:
      subscribe cbm-main-faq Firstname Lastname
      quit
      
  See Section 6 for directions on how to use these services to retrieve the
  FAQ.
  
  
   2.  Overview
  
  Obviously, we must walk before we run, and this principle applies to
  FAQ files as well.  Here are some general questions we often receive
  in the Commodore community. 
  
   
   2.1.  Do people still use Commodore 8-bit machines?
   
  Yes, people still do.  Newer machines may have appeared and taken over the
  corporate world, but the Commodore 8-bit machines live on.
  
   
   2.2.  How many Commodore machines are there?
  
  If you are asking the quantity of Commodore machines sold, the simple truth
  is that we do not know.  Commodore never officially released any such
  numbers for all models.  It has been estimated that Commodore sold
  over 10 million Commodore 64 machines, but that has not been proven, as far
  as I know.  So, if you ever determine exactly what quantity of each model
  was produced, please pass the information along.
   
  If you are asking the number of different models Commodore sold, we have
  a slightly better idea.  Jim Brain has compiled a list of all known CBM
  products, marketed or not, into the "Canonical List of Commodore Products".
  This include all of the Commodore line, including the PCs and the Amiga
  systems.  As it is much too large to fit in the FAQ, it can be requested 
  from Jim Brain's mailserver as file cbmmodel.txt (See Section 6.5.2 for
  directions on how to access the mailserver).  Alternately, the file is 
  posted to the USENET newsgroup comp.sys.cbm on a periodic basis.


   2.3.  What do people do with Commodore 8-bit machines?
   
  People use their machines for very different purposes:

        Game Console.
        Home Computer.
        Experimentor's machine.
        Small Business Computer.

  No matter what purpose they use there is a
  wealth of programs available for the Commodore computer systems.  The
  Commodore line of computers has a seemingly endless supply of quality
  programs available for it, and more are being created daily.

   
   2.4.  What Commodore 8-bit machines are most widely used?
   
     Well, it is a fact that all types of Commodore 8-bit computers are still
  in use, but the following machines get the most use:

        Commodore 64 (include SX64, DX64, and PET64)
        Commodore 128 (includes 128D and Euro 128D)

  The following systems manufactured by Commodore still have a devout
  following:

        Commodore VIC-20
        Commodore PET series
        Commodore B series
        Commodore Plus 4 and 16
        Commodore C65

+ The Commodore 65 (64DX)
  
  The Commodore 65 is a recent addition and is the result of a liquidation of
  some ALPHA stage test machines.  A number of people have purchased these
  test units, and they have a FAQ devoted just to this machine.  Much 
  information on this machine is available at 
  ftp://ccnga.uwaterloo.ca/pub/cbm/c65
  In spite of rumors, No company is considering manufacturing the C65.

| If you own a Commodore C65, the following people are compiling lists of
  people who own them.

  Robin Harbon
  542 West Donald Street.
  Thunder Bay, Ontario, P7E 5Y6
  Canada
  
+ Gary Pearson
+ gpearson@mistral.co.uk
  
+ The Commodore PET Series
  
  If you currently use a PET series Commodore computer or just want to know
  more about them, one person is trying to start a magazine devoted to these
  machine.  For more information or to submit articles for the magaziuch with:

  Mark J. Kingsbury
  25 Latta
  Battle Creek, MI  49017
  Mark_J_Kingsbury@fc1.glfn.org

+ If you own a Commodore VIC-20, the following individual is planning to
+ create a list of owners:

+ Jeff's Ink Press & Deli
+ P.O. Box 477493
+ Chicago IL  60647


   2.5.  What is the economic status of Commodore?
   
  On April 29, 1994, Commodore International announced that it had been unable
  to renegotiate terms of outstanding loans and were closing down the
  business.  In the months that followed, the liquidation process dragged on, 
  owing to the large far-reaching size of the corporation.  In addition, the
  fact that the company was incorporated in the Bahamas while a large share
  of the creditors were from the US made legal proceeding tense and drawn out.
  On April 20th, 1995, almost a full year later, Commodore was sold to
  a German ESCOM for approximately 10 to 12.5 million dollars.  
+ In early 1996, ESCOM annousell the Amiga technology to a
+ U.S. company called VISCorp, while reatining the Commodore name.  Then, in
+ July 1996, ESCOM announced that its was filing for bankruptcy protection
+ as it undergoes a reorganization process.  At present, the holder of the
+ CBM 8-bit technologies is unknown.
  
  Of course, since Commodore hasn't served the Commodore 8-bit community
  for quite some time, most Commodore owners are only interested in what
  will happen to Commodore Semiconductor Group (CSG), the fabricator for
  many of the special ICs in the Commodore 8-bit line.  Below is the current
  status of CSG as of April 6, 1995:

  Commodore Semiconductor Group liquidated in December, 1994.  The vast 
  majority of the operational material and the real estate was purchased by 
  GMT Electronics, a company formed by CSG's management.  GMT has paid the 
  $1 million lien that the EPA had levied against CSG, and is now operating 
  as a for-hire chip production plant.

  CSG/GMT is holding approximately $5 million in Commodore parts.

   
   3.  The BASICs
   
   These are some questions we receive about "BASIC", the built-in
   programming language in all 8-bit Commodore computers, and the "basics"
   of using the machine.
   
   
   3.1.  How do I format a Commodore disk?
   
  To format a disk in drive 0 (older PET drives had drive 0 and 1) on disk
  device #8, you issue the following command from BASIC:

  open1,8,15,"n0:16char_name,12":close1

| The name can be 16 characters in length, and the disk id (12 in this
  example) can be any two alphanumeric characters.

  For more information on how to use the 1541 disk drive or compatibles, 
  a complete manual is available at ftp://ftp.funet.fi/pub/cbm/documents.
  (See Section 6.9 for direction on how to use ftp.)
  
   
   3.2.  How do I transform a BASIC program to a text file?
   
  As you may know, Commodore BASIC stores programs in "tokenized" format,
  so they are unreadable from a standard text editor.  To fix that, load up
  you BASIC program, and then type the following in direct mode:

  open1,8,2,"listing,s,w":cmd1:list

  The text listing will be placed on drive 8 in a file called listing.  After
 finished, your cursor should return.  Type the following
  in:

  print#1:close1

  You now have an un-"tokenized" copy of your program, which you can edit with
  any text editor.

   
   3.3.  How do I transform a text file into a BASIC program?
   
  Since Commodore BASIC stores its programs in "tokenized" format, one
  cannot simply load text files containing BASIC statements and run the file
  directly.  However, there is a solution.  In direct mode, type in the 
  following:

  C64:
  open1,8,2,"filename":poke781,1:poke812,73:sys 65478
  
  C128:
  open1,8,2,"filename":sys 65478,,1

  This will read in each line of the text file and try to execute it (or 
  store it if the line is preceded by a number).  The screen will go blank
  (scroll upwards) while the file is retrieved and will likely end up 
  printing an error message, which is normal.  When the last line of
  the program is entered, hit RUN/STOP-RESTORE, and type in the following:

  close1

  The file will now be loaded into memory.  Immediately save the files a BASIC program.
  
  If the above sounds too complicated for you, check out the seq-to-basic
  prog comp.binaries.cbm every month.  It will perform
  the translation for you, after you answer a few simple prompts.


   3.4.  How can I change my drive device number through software?
  
  To change the device number on Commodore drives, follow these steps:
  In the following examples, 'olddn' is the drive's current device number,
  and 'newdn' is the new number you wish to change it to.
 
  1)    Turn off all drives except one you wish to change device number of.
  2)    Type the following in, depending on drive type:
 
    1540/41/42/4040/Most Compatibles:
        open 15,olddn,15
        print#15,"m-w"chr$(119)chr$(0)chr$(2)chr$(32+newdn)chr$(64+newdn)
        close 15

    MSD SD-1 (Old ROM):
        open 15,olddn,15
        print#15,"m-w"chr$(117)chr$(0)chr$(2)chr$(32+newdn)chr$(64+newdn)
        close 15
 
    1551/70/71/81
        open 15,olddn,15
        print#15,"u0>"+chr$(newdn)
        close 15
 
  3)    Turn back on other drives.
 
  The change is only temporary.  It will revert back if the drive is turned
  off.

   
   3.5.  Can I get my 1581 drive to change its device number on startup?
  
  When the 1581 is initialized, as well as checking the boot sector of the
  disk, it also looks for a file "copyright cbm 86".  This file, if found,
  can specify a device number for the 1581 disk.  Whenever the 1581 is booted
  or initialized with this disk inserted, its device number will be changed
  to the specified number.  The utility 1581-auto-dev by David W. Tamkin
  (can be found on ccnga.uwaterloo.ca in the utilities directory) will create
  this file.  It can also do other stuff, so check it out.
 

 

-- 
Jim Brain, Embedded System Designer, Brain Innovations, Inc. (BII)(offline sig)
j.brain@ieee.org   "Above views DO reflect my employer, since I'm my employer"
Dabbling in WWW, Embedded Systems, VR, Old CBM computers, and Good Times!  -Me-
<a href=http://www.msen.com/~brain/>Jim Brain: BII, VR, and CBM info</a>
